Sentry G3
Sentry G3 - 10 KVA
INPUT		
Rated power	10000 VA	
Frequency tolerance	 46-64 Hz or 56-64 Hz	
Power factor	  >0.99 @100% load	
OUTPUT and INVERTER OUTPUT		
Crest factor (Ipeak/Irms)	 3:1 	
Wave form on battery	Pure Sine Wave 	
BATTERIES		
Type	12V/9Ah 	
Recharge time	9 hours recovery to 9 hour capacity 	
Maximum recharge current	 8.0 A 	
ENVIRONMENTAL		
Safety compliance	EN 62040-1:2008; EN 62040-1/EC:2009; EN 62040-1/A1:2013 and Directive 2014/35/EU 	
EMC conformance	EN 62040-2 and Directive 2014/30/EU 	
Protection rating	IP20 	
Noise	Less than 58db@ 1 Meter 	
Relative humidity	0-95% RH @ 0-40 degree Celcius (non-condensing) 	
DATA		
Weight	38 kg	
Dimensions (h w d)	 826 x 250 x 592 mm