Master Switch Single Phase
MMS 32
INPUT		
Voltage	220 / 230 / 240 V single-phase + N 	
Voltage tolerance	180-264 (selectable) 	
Frequency tolerance	±10% (selectable)	
Input frequency	50 / 60 Hz	
Switched input phases	ph+N (two poles) 	
Distribution compatibility	IT, TT, TNS, TNC	
ENVIRONMENTAL		
Color	RAL 7016 	
Protection rating	IP20 	
Other compliances	EN 62310-1 (safety) EN 62310-2 (electro-magnetic compatibility) 	
Noise	< 40 dBA 	
Operating temperature	0 °C - +40 °C	
Storing temperature	-10 °C up to +50 °C	
Relative humidity	5-95% non-condensing	
Transport	“Break Before Make” (no overlapping sources) 	
Available transfer modes	Automatic / Manual / Remote	
DATA		
Weight	10 kg	
Dimensions (h w d)	2U x 19” x 520 mm