Multi Guard Industrial
GMI 160 (M)
INPUT		
Voltage	380 / 400 / 415 V three-phase + N and 220 / 230 / 240 V single-phase + N (input voltage recognition function) 	
Voltage tolerance	230 / 400 ±20% @ full load 	
Frequency tolerance	40-72 Hz	
Power factor	>0.99	
Current distorsion	< 3%	
BY PASS		
Rated voltage	220 / 230 / 240 V , single-phase + N	
Voltage tolerance	180 / 264 V (selectable) referring to neutral phase 	
OUTPUT and INVERTER OUTPUT		
Rated power	20000 VA	
Active power	18000 W	
Frequency	50 / 60 Hz 	
BATTERIES		
Type	VRLA AGM/GEL 	
Recharge time	6 hours 	
ENVIRONMENTAL		
Color	Light gray RAL 7035 	
Protection rating	IP20 	
Noise	from ≤ 52 dBA to ≤ 70 dBA 	
Operating temperature	0 °C - +40 °C	
Storing temperature	-15 °C +55 °C	
Relative humidity	20% - 90% non-condensing	
Standards	European directives: L V 2014/35/EU low voltage; EMC 2014/30/EU electromagnetic compatibility -- Directive and Standards: Safety IEC EN 62040-1; EMC IEC EN 62040-2; RoHS compliant -- Classification in accordance with IEC 62040-3 VFI - SS - 111 	
DATA		
Weight	200 (UPS modules excluded) kg	
Dimensions (h w d)	2060 x 850 x 850 mm