Multi Switch ATS
MTA 30A
INPUT		
Voltage	180-264 (selectable) 	
Frequency	50 / 60 Hz 	
ENVIRONMENTAL		
Color	RAL 5004 	
Communication	RS232 / USB / Slot for communication interface / Relay contacts port 	
Protection rating	IP20 	
Other compliances	EN 62310-1 (safety) EN 62310-2 (electro-magnetic compatibility) 	
Protections	Overcurrent - overvoltage - undervoltage - protection against energy back-feed	
Noise	< 35 dBA 	
Operating temperature	0 °C - +40 °C	
Storing temperature	-10 °C up to +50 °C	
Relative humidity	5-95% non-condensing	
Output sockets	30 A on Terminal board and 4 IEC-320 C13 (10 A) + 1 IEC-320 C19 (16 A) 	
DATA		
Weight	5 kg	
Dimensions (h w d)	1U x 19” x 330 mm