SPH
SPM 6 ER
OVERALL SPECIFICATION		
Output power factor [pf]	0.9 	
INPUT		
Voltage tolerance	220-230-240 Vac ± 20% 	
Frequency tolerance	±10 Hz	
Input frequency	50/60 Hz	
BY PASS		
Voltage tolerance	160 -276 Vac (Selectable in Eco Mode or Smart Active Mode) 	
Frequency tolerance	Selected frequency ±10% 	
OUTPUT and INVERTER OUTPUT		
Number phases	Single Phase 	
Crest factor (Ipeak/Irms)	3:1 	
Waveform (Battery Mode)	Sinusoidal 	
Frequency	50/60 Hz selectable or with automatic selection 	
Load power factor	0.9 	
BATTERIES		
Type	VRLA AGM maintenance-free lead based 	
ENVIRONMENTAL		
Color	Dark grey RAL 7016 	
Communication	USB / R232 + slot for communication interface 	
Safety compliance	EN 62040-1 	
EMC conformance	EN 62040-2 Directives 2006/95/EC - 2004/108 	
Marks	CE 	
Other compliances	BIS Registered 	
Noise	< 40 dBA 	
Operating temperature	0 °C / +40 °C	
Relative humidity	< 95% non-condensing	
DATA		
Weight	25.5 kg	
Dimensions (h w d)	262X654X709 mm	
Input phases	Single Phase 	
Output phases	Single Phase