Sentryum
S3M 10 CPT
INPUT		
Rated power	10000 VA	
Voltage	380 / 400 / 415 V three-phase + N - 220 / 230 / 240 V single-phase + N 	
Voltage tolerance	230 / 400 V ±20% @ full load (for wider tolerance conditions apply) 	
Frequency tolerance	40 - 72 Hz	
Power factor	0.99	
BY PASS		
Rated voltage	220 / 230 / 240 V single-phase + N	
Voltage tolerance	From 180 V (adjustable 180-200) to 264 V (adjustable 250-264) referring to neutral (Ph-N) 	
Rated frequency	50 or 60 Hz (selectable) 	
Frequency tolerance	±5% (selectable) 	
Number phases	1 + N 	
OUTPUT and INVERTER OUTPUT		
Rated power	10000 VA	
Active power	10000 W	
Output current	48 (bypass) A - 43 (inverter) A	
Number phases	1 + N 	
Crest factor (Ipeak/Irms)	3 : 1 	
Waveform (Battery Mode)	Sinusoidal 	
Static stability	±0.5% 	
Dynamic stability	EN 62040-3 class performance 1 non-linear load 	
Frequency	50 or 60 Hz 	
Voltage distortion with non-linear load	≤1.5% 	
Voltage distortion with linear load	<1% 	
BATTERIES		
Type	VRLA AGM/GEL/NiCd/Li-ion/Supercaps 	
Type of charging	One level, Two level, Cyclic recharge (selectable) 	
ENVIRONMENTAL		
Color	RAL 7016 	
Communication	UPS status led bar - Graphic touch screen display - 2 slots for communications interface USB - RS232 - Contact interface with 5x opto insulated Input and 4x Output relays 	
Protection rating	IP20 	
Line-Interactive/Smart Active efficiency	Up to 99% 	
Noise	<40 [dBA ±2] (SMART ACTIVE) 	
Remote signals	voltage free contacts	
Operating temperature	0 °C - +40 °C	
Relative humidity	5-95% non-condensing	
Standards	European directives: LV 2014/35/EU low voltage; EMC 2014/30/EU electromagnetic compatibility -- Directive and Standards: Safety IEC EN 62040-1; EMC IEC EN 62040-2; RoHS compliant -- Classification in accordance with IEC EN 62040-3 VFI - SS - 111 	
DATA		
Weight	48 kg	
Dimensions (h w d)	700x280x840 mm